FLOTSAM MODIFICATION LIST (FROM A1)

* REMOVE SOLDERPASTE OPENINGS FOR TP
* UPDATE TANT CAP FOOTPRINT TO ADD POLARITY SILKSCREEN
* REMOVE GND HOOK FROM BOM
* ADD LEVEL TRANSLATOR FOR I2C BUS